Use this editable response form for C2 bids. Add/remove rows as needed, but keep each bid within the correct category and sub-category. For equivalent products, you may replace the requested product with the product you plan to bid. Please notate where you are not bidding.

**Fill out form and include with your bid**

**\*\*\* REQUESTING PROPOSALS FOR MANUFACTURER AND PART NUMBER LISTED. EQUIVALENT OR SUPERIOR\*\*\***

***\*Complete this form including all proposed components, itemized costs, E-Rate eligibility, and service/design/installation costs as separate line items. Responses should at a minimum include the required components as requested within the RFP, but should be amended to include any additional/alternate materials/resources/components which the vendor believes is necessary to provide a complete functioning solution. Responses which include additional/alternate components must include an explanation for such changes. \*\*This response form must be provided in digital, Microsoft Word or Excel format. Hard copies will be accepted but NOT IN EXCLUSION OF THE DIGITAL COPY.***

| **Item Number/Description** | **Qty** | **Unit Cost** | **Extended Cost** | **E-Rate Eligibility (Y/N)** | **E-Rate Eligible Amount** |
| --- | --- | --- | --- | --- | --- |
| ***ARLINGTON CAMPUS*** |  |  |  |  |  |
| **Wireless Networking** |  |  |  |  |  |
| **Meraki CW9164** | **63** |  |  |  |  |
| **Meraki CW9166** | **1** |  |  |  |  |
| **MR License** | **64** |  |  |  |  |
| **\*Installation** |  |  |  |  |  |
| **Network Data Cabling** |  |  |  |  |  |
| **CAT6a Network Data Cabling** | **64** |  |  |  |  |
| **CAT6 Network Data Cabling**  | **252** |  |  |  |  |
| **CAT6 Smart Board Data Cabling**  | **54** |  |  |  |  |
| **CAT6a Yellow Patch Cables (10ft)**  | **64** |  |  |  |  |
| **CAT6a Yellow Patch Cables (8in)**  | **64** |  |  |  |  |
| **CAT6 Blue Patch Cables (10ft)**  | **252** |  |  |  |  |
| **CAT6 Blue Patch Cables (8in)**  | **252** |  |  |  |  |
| **CAT6 Orange Patch Cables (10ft)**  | **54** |  |  |  |  |
| **CAT6 Orange Patch Cables (8in)**  | **54** |  |  |  |  |
| **Modular Patch Panel 48-Port**  | **13** |  |  |  |  |
| **Modular Patch Panel 24-Port**  | **1** |  |  |  |  |
| **HPE G2 Enterprise Pallet Rack**  | **2** |  |  |  |  |
| **MM Fiber, 12-Strand, OM4**  | **1** |  |  |  |  |
| **500i SDX Fiber Shelf**  | **2** |  |  |  |  |
| **OM4 12-Fiber Adapter Panel LC**  | **2** |  |  |  |  |
| **LC to LC OM4 MMF 3m Patch Cable**  | **12** |  |  |  |  |
| **\*Engineering/Design**  |  |  |  |  |  |
| **\*Installation/Implementation** |  |  |  |  |  |
| **U**ninterruptable Power Supply |  |  |  |  |  |
| **APC Smart-UPS Line Interactive, 3kVA Li-Ion Rackmount 2U, 120V, 2X NEMA 5-20R+6x NEMA 5-15R outlets, SmartConnect Port+Network Card, AVR, LCD**  | **2** |  |  |  |  |
| **HPE G2 Metered/Switched Vertical Full-Height PDU**  | **4** |  |  |  |  |
| ***GRAND PRAIRIE CAMPUS*** |  |  |  |  |  |
| **Wireless Networking** |  |  |  |  |  |
| **Meraki CW9164** | **63** |  |  |  |  |
| **Meraki CW9166** | **1** |  |  |  |  |
| **MR License** | **64** |  |  |  |  |
| **\*Installation** |  |  |  |  |  |
| **Network Data Cabling** |  |  |  |  |  |
| **CAT6a Network Data Cabling** | **64** |  |  |  |  |
| **CAT6 Network Data Cabling**  | **252** |  |  |  |  |
| **CAT6 Smart Board Data Cabling**  | **54** |  |  |  |  |
| **CAT6a Yellow Patch Cables (10ft)**  | **64** |  |  |  |  |
| **CAT6a Yellow Patch Cables (8in)**  | **64** |  |  |  |  |
| **CAT6 Blue Patch Cables (10ft)**  | **252** |  |  |  |  |
| **CAT6 Blue Patch Cables (8in)**  | **252** |  |  |  |  |
| **CAT6 Orange Patch Cables (10ft)**  | **54** |  |  |  |  |
| **CAT6 Orange Patch Cables (8in)**  | **54** |  |  |  |  |
| **Modular Patch Panel 48-Port**  | **13** |  |  |  |  |
| **Modular Patch Panel 24-Port**  | **1** |  |  |  |  |
| **HPE G2 Enterprise Pallet Rack**  | **2** |  |  |  |  |
| **MM Fiber, 12-Strand, OM4**  | **1** |  |  |  |  |
| **500i SDX Fiber Shelf**  | **2** |  |  |  |  |
| **OM4 12-Fiber Adapter Panel LC**  | **2** |  |  |  |  |
| **LC to LC OM4 MMF 3m Patch Cable**  | **12** |  |  |  |  |
| **\*Engineering/Design**  |  |  |  |  |  |
| **\*Installation/Implementation** |  |  |  |  |  |
| **U**ninterruptable Power Supply |  |  |  |  |  |
| **APC Smart-UPS Line Interactive, 3kVA Li-Ion Rackmount 2U, 120V, 2X NEMA 5-20R+6x NEMA 5-15R outlets, SmartConnect Port+Network Card, AVR, LCD**  | **2** |  |  |  |  |
| **HPE G2 Metered/Switched Vertical Full-Height PDU**  | **4** |  |  |  |  |